# Weather and Climate Inputs for 'SWAT'

## Documentation for package ‘wcswatin’ version 0.1.1

- DESCRIPTION file
- User guides, package vignettes and other documentation
- Package NEWS
- Package README

## Help Pages

wcswatin-package | wcswatin: Climate & Weather SWAT Input.
character-raster | Input Raster
count_na | Count the amount or percentage of 'NA' in a table by column
cube2table | Convert a Cube format data into a Table format
daily_aggregation | Create a daily aggregation from an hourly dataset
datacube_aggregation | Create a daily aggregation from an hourly datacube
files_to_table | Turns multiple time series files into a single table
fill_gap | A wrapper function for filling gaps in the rainfall time series
input_raster | Input Raster
input_raster-method | Input Raster
layervalues2pixel | Series of Pixel Values
main_input_var | Main table constructor by Variable
point_to_daily | Transforms the raw value from point perspective to a daily perspective
RasterBrick | Input Raster
RasterLayer | Input Raster
RasterStack | Input Raster
raster_info | Summarize raster file metadata
rh_calculator | Calculate the Relative Humidity from dewpoint and ambient temperature
save_daily_tbl | Save the csv files after transformation to daily form
SpatRaster | Input Raster
study_area_records | Study Area Records
summary_plot | Plot a summary of the data
summary_table | Table summary of the data
table_to_files | Export tables to 'txt' or 'csv' files
tbl_from_references | Extract gridded values at station or reference points
ts_point_to_files | Save trend-surface point time series to files
ts_to_area | Trend Surface Interpolation into Raster
ts_to_point | Trend Surface Interpolation into Targeded Points
unit_converter | Unit Converter
var_main_creator | Main table creator for SWAT Input from Trend SUrface Interpolation
var_names | Shows raster variables present in a NetCDF
wcswatin | wcswatin: Climate & Weather SWAT Input.
windspeed_calculator | Calculate the wind speed from Eastward and Northward Near-Surface Wind